The recommended two-way route south of the traffic separation scheme (TSS) formalizes traffic patterns where slower vessels such as tug and barge traffic and fishing vessels pass starboard to starboard.  Slower moving traffic transiting eastbound should follow the route established south of the TSS and north of the recommended two-way route line depicted.  Slower moving traffic transiting westbound should follow the route established south of the recommended two-way route line.