NOAA ENCŪ

NATIONAL OCEANIC AND ATMOSPHERIC ADMINISTRATION

US5CA44M - SAN JOAQUIN RIVER; STOCKTON DEEP WATER CHANNEL; ANTIOCH TO MEDFORD ISLAND


INDEX:

NOTE A
NOTE C
AIDS TO NAVIGATION
AUTHORITIES
POLLUTION REPORTS
BRIDGE AND OVERHEAD CABLE CLEARANCES
CAUTION - LIMITATIONS
SUPPLEMENTAL INFORMATION
RADAR REFLECTORS
CAUTION - TEMPORARY CHANGES
CAUTION - DREDGED AREAS
USACE HYDROGRAPHIC SURVEYS
NOAA WEATHER RADIO BROADCASTS
CAUTION - SUBMARINE PIPELINE AND CABLES
RULES OF THE ROAD (ABRIDGED)
CAUTION - WARNING CONCERNING LARGE VESSELS
CAUTION - SMALL CRAFT
WARNING - PRUDENT MARINER
ADMINISTRATION AREA
WATER LEVELS, CURRENTS, AND TIDES
ADDITIONAL INFORMATION
COMMENTS REQUESTED


NOTES:

NOTE A
Navigation regulations are published in Chapter 2, U.S. Coast Pilot 7.  Additions or revisions to Chapter 2 are published in the Notice to Mariners. Information concerning the regulations may be obtained at the Office of the Commander, 11th Coast Guard District in Alameda, California or at the Office of the District Engineer, Corps of Engineers in Sacramento, California.
Refer to charted regulation section numbers.


NOTE C
The U.S. Coast Guard operates a mandatory Vessel Traffic Services (VTS) system in the San Francisco Bay and surrounding areas. Vessel operating procedures and designated radiotelephone frequencies are published in 33 CFR 161, the U.S. Coast Pilot, and/or the VTS User's Manual. The entire area of the chart falls within the Vessel Traffic Services (VTS) system.


AIDS TO NAVIGATION
Consult U.S. Coast Guard Light List for supplemental information concerning aids to navigation.


AUTHORITIES
Hydrography and topography by the National Ocean Service, Coast Survey, with additional data from the Corps of Engineers, Geological Survey, and U.S. Coast Guard.


POLLUTION REPORTS
Report all spills of oil and hazardous substances to the National Response Center via 1-800-424-8802 (toll free), or to the nearest U.S. Coast Guard facility if telephone communication is impossible (33 CFR 153).


BRIDGE AND OVERHEAD CABLE CLEARANCES
Clearances are charted as furnished by the Corps of Engineers and U.S. Coast Guard. Overhead cable clearances are referred to high water. Bridge clearances are referred to High Water (HW) and Low Water (LW).


CAUTION - LIMITATIONS
Limitations on the use of radio signals as aids to marine navigation can be found in the U.S. Coast Guard Light Lists and National Geospatial-Intelligence Agency Publication 117. Radio direction-finder bearings to commercial broadcasting stations are subject to error and should be used with caution.


SUPPLEMENTAL INFORMATION
Consult U.S. Coast Pilot 7 for important supplemental information.


RADAR REFLECTORS 
Radar reflectors have been placed on many floating aids to navigation. Individual radar reflector identification on these aids has been omitted from this chart.


CAUTION - TEMPORARY CHANGES
Temporary changes or defects in aids to navigation are not indicated. See Local Notice to Mariners.


CAUTION - DREDGED AREAS
Improved channels are subject to shoaling, particularly at the edges.


USACE HYDROGRAPHIC SURVEYS
USACE conducts hydrographic surveys to monitor navigation conditions. These surveys are not intended to detect underwater features. Uncharted features hazardous to surface navigation are not expected but may exist in federal channels. For more information visit https://navigation.usace.army.mil/Survey/Hydro/ .


NOAA WEATHER RADIO BROADCASTS
The NOAA Weather Radio stations listed below provide continuous weather broadcasts. The reception range is typically 20 to 40 nautical miles from the antenna site, but can be as much as 100 nautical miles for stations at high elevations.

Mt. Pise, CA           KHB-49     162.40 MHz WX2
Sacramento, CA         KEC-57      162.55 MHz WX1


CAUTION - SUBMARINE PIPELINE AND CABLES
Additional uncharted submarine pipelines and submarine cables may exist within the area of this chart. Not all submarine pipelines and submarine cables are required to be buried, and those that were originally buried may have become exposed. Mariners should use extreme caution when operating vessels in depths of water comparable to their draft in areas where pipelines and cables may exist, and when anchoring, dragging, or trawling. Covered wells may be marked by lighted or unlighted buoys.


RULES OF THE ROAD (ABRIDGED)
Motorless craft have the right-of-way in almost all cases. Sailing vessels and motorboats less than 19.8 meters/65 feet in length shall not hamper, in a narrow channel, the safe passage of a vessel which can navigate only inside that channel. A motorboat being overtaken has the right-of-way. Motorboats approaching head to head or nearly so should pass port to port. When motorboats approach each other at right angles or obliquely, the boat on the right has the right-of-way in most cases. Motorboats must keep to the right in narrow channels when safe and practicable. Mariners are urged to become familiar with the complete text of the Rules of the Road in U.S. Coast Guard publication "Navigation Rules."


CAUTION - WARNING CONCERNING LARGE VESSELS
The "Rules of the Road" state that recreational boats shall not impede the passage of a vessel that can navigate only within a narrow channel or fairway. Large vessels may appear to move slowly due to their large size but actually transit at speeds in excess of 22.2 kilometers per hour/12 knots, requiring a great distance in which to maneuver or stop. A large vessel's superstructure may block the wind with the result that sailboats and sailboards may unexpectedly find themselves unable to maneuver. Bow and stern waves can be hazardous to small vessels. Large vessels may not be able to see small craft close to their bows.


CAUTION - SMALL CRAFT
Small craft should stay clear of large commercial and government vessels even if small craft have the right-of-way. All craft should avoid areas where the skin divers flag, a red square with a diagonal white stripe, is displayed.


WARNING - PRUDENT MARINER
The prudent mariner will not rely solely on any single aid to navigation, particularly on floating aids. See U.S. Coast Guard Light List and U.S. Coast Pilot for details.


ADMINISTRATION AREA
The entire extent of this ENC cell falls within the limits of an Administration Area. This area covers land, internal waters and territorial sea. The territorial sea is a maritime zone over which the United States exercises sovereignty extending to the airspace as well as to its bed and subsoil. For more information, please refer to the Coast Pilot.


WATER LEVELS, CURRENTS, AND TIDES
Real-time water levels, tide predictions, and tidal current predictions are available on the internet from NOAA's Center for Operational Oceanographic Products and Services (CO-OPS) at https://tidesandcurrents.noaa.gov/water_level_info.html and https://tidesandcurrents.noaa.gov/currents_info.html.


ADDITIONAL INFORMATION
Additional information can be obtained at www.nauticalcharts.noaa.gov.


COMMENTS REQUESTED
NOAA encourages users to submit inquiries, discrepancies, or comments about this chart via NOAA's ASSIST tool at https://www.nauticalcharts.noaa.gov/customer-service/assist/.


END OF FILE